Introspection Runtime Mode = true

========================================
csvStg1:
Number,Name,Version,State,Reference Designators,Line Number,Find Number,Quantity,phValue,phRohsStatus,phManufacturingTechnology,phTolNegPercent,phTolPosPercent


========================================
txtStg1:
Number;Name;Version;State;Reference Designators;Line Number;Find Number;Quantity;phValue;phRohsStatus;phManufacturingTechnology;phTolNegPercent;phTolPosPercent

CSV File Path: C:\tmp\wtp_uses_attr\CC111111111_092810_161001.csv

TXT File Path: C:\tmp\wtp_uses_attr\CC111111111_092810_161001.txt


========================================
csvStg2:
Number,Name,Version,State,Reference Designators,Line Number,Find Number,Quantity,phValue,phRohsStatus,phManufacturingTechnology,phTolNegPercent,phTolPosPercent
CC111111111,myBom-1,1.137,PROTOTYPEINWORK,null,null,null,0.0,

========================================
txtStg2:
Number;Name;Version;State;Reference Designators;Line Number;Find Number;Quantity;phValue;phRohsStatus;phManufacturingTechnology;phTolNegPercent;phTolPosPercent
CC111111111;myBom-1;1.137;PROTOTYPEINWORK;null;null;null;0.0;
***attrFullStgArr[d]=: phManufacturingTechnology:BULK-ITEM = getStgArr[e]: phManufacturingTechnology

***attrFullStgArr[d]=: phValue:48V RECT = getStgArr[e]: phValue

***attrFullStgArr[d]=: phRohsStatus:25 = getStgArr[e]: phRohsStatus

occur.size(): 1
csvRefDes: V7 V8 V9

txtRefDes: V7,V8,V9

wtpartusagelink.getQuantity().getUnit(): ea

wtpartusagelink.getLineNumber().toString: 1


========================================
csvStg+:
Number,Name,Version,State,Reference Designators,Line Number,Find Number,Quantity,phValue,phRohsStatus,phManufacturingTechnology,phTolNegPercent,phTolPosPercent
CC111111111,myBom-1,1.137,PROTOTYPEINWORK,null,null,null,0.0,BULK-ITEM,48V RECT,25,
CC408639537,THYR SKKT 106B16 E G6,1.2,RELEASED,V7 V8 V9,1,,3.0,

========================================
txtStg+:
Number;Name;Version;State;Reference Designators;Line Number;Find Number;Quantity;phValue;phRohsStatus;phManufacturingTechnology;phTolNegPercent;phTolPosPercent
CC111111111;myBom-1;1.137;PROTOTYPEINWORK;null;null;null;0.0;BULK-ITEM;48V RECT;25;
CC408639537;THYR SKKT 106B16 E G6;1.2;RELEASED;V7,V8,V9;1;;3.0;
***attrFullStgArr[d]=: phManufacturingTechnology:SELECT A VALUE = getStgArr[e]: phManufacturingTechnology

***attrFullStgArr[d]=: phValue:ENTER A VALUE = getStgArr[e]: phValue

***attrFullStgArr[d]=: phRohsStatus:TBD = getStgArr[e]: phRohsStatus

occur.size(): 1
csvRefDes: V7 V8 V9

txtRefDes: V7,V8,V9

occur.size(): 1
csvRefDes: V1 V2 V3

txtRefDes: V1,V2,V3

wtpartusagelink.getQuantity().getUnit(): ea

wtpartusagelink.getLineNumber().toString: 3


========================================
csvStg+:
Number,Name,Version,State,Reference Designators,Line Number,Find Number,Quantity,phValue,phRohsStatus,phManufacturingTechnology,phTolNegPercent,phTolPosPercent
CC111111111,myBom-1,1.137,PROTOTYPEINWORK,null,null,null,0.0,BULK-ITEM,48V RECT,25,
CC408639537,THYR SKKT 106B16 E G6,1.2,RELEASED,V7 V8 V9,1,,3.0,SELECT A VALUE,ENTER A VALUE,TBD,
CC408624407,THYR MD7LC5716E,1.3,RELEASED,V1 V2 V3,3,,3.0,

========================================
txtStg+:
Number;Name;Version;State;Reference Designators;Line Number;Find Number;Quantity;phValue;phRohsStatus;phManufacturingTechnology;phTolNegPercent;phTolPosPercent
CC111111111;myBom-1;1.137;PROTOTYPEINWORK;null;null;null;0.0;BULK-ITEM;48V RECT;25;
CC408639537;THYR SKKT 106B16 E G6;1.2;RELEASED;V7,V8,V9;1;;3.0;SELECT A VALUE;ENTER A VALUE;TBD;
CC408624407;THYR MD7LC5716E;1.3;RELEASED;V1,V2,V3;3;;3.0;
***attrFullStgArr[d]=: phManufacturingTechnology:HAND = getStgArr[e]: phManufacturingTechnology

***attrFullStgArr[d]=: phValue:ENTER A VALUE = getStgArr[e]: phValue

***attrFullStgArr[d]=: phRohsStatus:N = getStgArr[e]: phRohsStatus

occur.size(): 1
csvRefDes: V1 V2 V3

txtRefDes: V1,V2,V3

occur.size(): 0
csvRefDes: 

txtRefDes: 

wtpartusagelink.getQuantity().getUnit(): G


========================================
csvStg+:
Number,Name,Version,State,Reference Designators,Line Number,Find Number,Quantity,phValue,phRohsStatus,phManufacturingTechnology,phTolNegPercent,phTolPosPercent
CC111111111,myBom-1,1.137,PROTOTYPEINWORK,null,null,null,0.0,BULK-ITEM,48V RECT,25,
CC408639537,THYR SKKT 106B16 E G6,1.2,RELEASED,V7 V8 V9,1,,3.0,SELECT A VALUE,ENTER A VALUE,TBD,
CC408624407,THYR MD7LC5716E,1.3,RELEASED,V1 V2 V3,3,,3.0,HAND,ENTER A VALUE,N,
850000255,SolderPasteTest,1.6,RELEASED,,,,1.5,

========================================
txtStg+:
Number;Name;Version;State;Reference Designators;Line Number;Find Number;Quantity;phValue;phRohsStatus;phManufacturingTechnology;phTolNegPercent;phTolPosPercent
CC111111111;myBom-1;1.137;PROTOTYPEINWORK;null;null;null;0.0;BULK-ITEM;48V RECT;25;
CC408639537;THYR SKKT 106B16 E G6;1.2;RELEASED;V7,V8,V9;1;;3.0;SELECT A VALUE;ENTER A VALUE;TBD;
CC408624407;THYR MD7LC5716E;1.3;RELEASED;V1,V2,V3;3;;3.0;HAND;ENTER A VALUE;N;
850000255;SolderPasteTest;1.6;RELEASED;;;;1.5;
***attrFullStgArr[d]=: phManufacturingTechnology:HAND = getStgArr[e]: phManufacturingTechnology

***attrFullStgArr[d]=: phValue:Lead-free = getStgArr[e]: phValue

***attrFullStgArr[d]=: phTolNegPercent:0.0000000000000 = getStgArr[e]: phTolNegPercent

***attrFullStgArr[d]=: phTolPosPercent:0.0000000000000 = getStgArr[e]: phTolPosPercent

occur.size(): 0
csvRefDes: 

txtRefDes: 

Got Out, ready to create csv file: C:\tmp\wtp_uses_attr\CC111111111_092810_161001.csv
Got Out, ready to create txt file: C:\tmp\wtp_uses_attr\CC111111111_092810_161001.txt
1 Objects Queried.
